{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Facility Summary","Year Summary","Emission Factors"],"not_rendered":{"charts":3,"images":2,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Facility Summary","index":0,"n_rows":15,"n_cols":16,"rows_kept":15,"cut":false,"hidden":false,"merged":[[10,1,10,16],[13,3,13,4],[13,6,13,7],[13,9,13,10],[13,12,13,13],[13,15,13,16],[13,1,14,1],[14,3,14,4],[14,6,14,7],[14,9,14,10],[14,12,14,13],[14,15,14,16]]}
[]
[null,"[Enter Organization Name]"]
[null,"Greenhouse Gas Emissions Tracking Spreadsheet"]
[null,"Facility Summary"]
[null,"Facilities:",0]
[]
[]
[]
[]
[]
[null,"Solid Waste Management Organization Summary "]
[null,"All values are in metric tons of CO2-e"]
[]
[null,"Facility",null,"Scope 1",null,null,"Scope 2",null,null,"Scope 3",null,null,"Scope 1+2",null,null,"Scope 1+2+3"]
[null,null,null,{"$f":"SUM(D16:E1048576)","v":0},null,null,{"$f":"SUM(G16:H1048576)","v":0},null,null,{"$f":"SUM(J16:K1048576)","v":0},null,null,{"$f":"SUM(M16:N1048576)","v":0},null,null,{"$f":"SUM(P16:Q1048576)","v":0}]

{"sheet":"Year Summary","index":1,"n_rows":15,"n_cols":27,"rows_kept":15,"cut":false,"hidden":false,"merged":[[14,12,14,13],[14,15,14,16],[10,1,10,16],[13,1,14,1],[13,3,13,4],[13,6,13,7],[13,9,13,10],[13,12,13,13],[13,15,13,16],[14,3,14,4],[14,6,14,7],[14,9,14,10]]}
[]
[null,{"$f":"'Facility Summary'!$B$2","v":"[Enter Organization Name]"}]
[null,"Greenhouse Gas Emissions Tracking Spreadsheet"]
[null,"Year Summary"]
[null,"Facilities:",0]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[]
[]
[]
[null,"Solid Waste Management Organization Summary "]
[null,"All values are in metric tons of CO2-e"]
[]
[null,"Year",null,"Scope 1",null,null,"Scope 2",null,null,"Scope 3",null,null,"Scope 1+2",null,null,"Scope 1+2+3"]
[null,null,null,{"$f":"SUM(D16:D1048576)","v":0},null,null,{"$f":"SUM(G16:G1048576)","v":0},null,null,{"$f":"SUM(J16:J1048576)","v":0},null,null,{"$f":"SUM(M16:M1048576)","v":0},null,null,{"$f":"SUM(P16:P1048576)","v":0}]

{"sheet":"Emission Factors","index":2,"n_rows":491,"n_cols":13,"rows_kept":491,"cut":false,"hidden":false,"merged":[[481,4,485,4],[486,4,489,4],[443,6,444,6],[445,4,448,4],[449,4,452,4],[453,4,456,4],[457,4,460,4],[461,4,465,4],[466,4,470,4],[471,4,475,4],[476,4,480,4],[410,4,414,4],[415,4,419,4],[420,4,424,4],[425,4,429,4],[430,4,434,4],[435,4,438,4],[442,0,442,2],[443,4,444,4],[443,5,444,5],[391,0,391,2],[392,4,393,4],[392,5,393,5],[392,6,393,6],[394,4,397,4],[398,4,401,4],[402,4,405,4],[406,4,409,4],[375,2,375,3],[7,12,7,19],[228,0,229,0],[228,1,229,1],[228,2,229,2],[286,4,286,8],[289,0,289,2],[326,0,326,2],[337,4,337,8],[341,0,341,2],[219,4,220,8],[261,4,261,8],[262,4,262,8],[265,4,266,4],[265,5,266,5],[228,4,229,4],[228,5,229,5],[290,4,291,4],[290,5,291,5],[168,8,168,9],[169,8,169,9],[136,4,137,4],[136,8,137,9],[156,8,156,9],[157,4,159,9],[77,0,77,2],[78,0,79,0],[78,1,79,1],[78,2,79,2],[135,0,135,2],[136,0,137,0],[136,1,137,1],[163,0,164,0],[163,1,164,1],[163,2,164,2],[91,0,91,2],[108,0,109,0],[108,1,109,1],[108,2,109,2],[127,0,128,0],[127,1,128,1],[127,2,128,2],[154,0,155,0],[154,1,155,1],[154,2,155,2],[145,0,146,0],[145,1,146,1],[145,2,146,2],[99,0,99,2],[100,0,101,0],[100,1,101,1],[100,2,101,2],[92,0,93,0],[215,0,216,0],[215,1,216,1],[215,2,216,2],[130,4,131,9],[215,4,216,4],[215,5,216,5],[92,1,93,1],[92,2,93,2],[92,4,93,4],[92,8,93,9],[94,8,94,9],[116,8,116,9],[117,8,117,9],[207,0,207,5],[136,2,137,2],[163,4,164,4],[118,8,118,9],[119,8,119,9],[120,8,120,9],[110,8,110,9],[17,0,18,0],[17,1,18,1],[17,2,18,2],[17,4,18,4],[17,8,18,8],[17,9,18,9],[54,8,54,9],[55,4,57,9],[65,0,66,0],[65,1,66,1],[65,2,66,2],[52,0,53,0],[52,1,53,1],[47,4,48,9],[65,4,66,4],[65,8,66,9],[0,12,0,19],[1,12,1,19],[2,12,2,19],[3,12,3,19],[4,12,4,19],[5,12,5,19],[6,12,6,19],[359,2,359,3],[46,4,46,9],[52,2,53,2],[52,4,53,4],[52,8,53,9],[70,8,70,9],[70,10,70,11],[71,8,71,9],[71,10,71,11],[65,10,66,11],[67,8,67,9],[67,10,67,11],[68,8,68,9],[323,4,323,8],[324,4,324,8],[342,4,343,4],[83,8,83,9],[374,2,374,3],[372,2,372,3],[373,2,373,3],[355,0,357,0],[356,2,356,3],[357,2,357,3],[355,2,355,3],[358,2,358,3],[365,2,365,3],[363,2,363,3],[370,2,370,3],[371,2,371,3],[368,2,368,3],[369,2,369,3],[366,2,366,3],[367,2,367,3],[364,2,364,3],[362,2,362,3],[360,2,360,3],[361,2,361,3],[83,10,83,11],[84,8,84,9],[84,10,84,11],[85,4,88,9],[102,8,102,9],[103,4,104,9],[108,4,109,4],[108,8,109,9],[68,10,68,11],[69,8,69,9],[69,10,69,11],[80,10,80,11],[81,8,81,9],[81,10,81,11],[82,8,82,9],[82,10,82,11],[78,4,79,4],[78,8,79,9],[78,10,79,11],[72,4,74,9],[100,4,101,4],[100,8,101,9],[80,8,80,9],[95,4,96,9],[111,8,111,9],[112,8,112,9],[113,8,113,9],[114,8,114,9],[115,8,115,9],[342,5,343,5],[327,4,328,4],[327,5,328,5],[342,7,343,7],[127,4,128,4],[127,8,128,9],[154,4,155,4],[154,8,155,9],[138,8,138,9],[139,4,141,9],[145,4,146,4],[145,8,146,9],[189,4,191,9],[181,0,182,0],[181,1,182,1],[181,2,182,2],[181,4,182,4],[181,8,182,9],[170,8,170,9],[121,8,121,9],[129,8,129,9],[122,4,123,9],[147,8,147,9],[148,4,150,9],[165,8,165,9],[166,8,166,9],[167,8,167,9],[163,8,164,9],[171,8,171,9],[172,8,172,9],[173,8,173,9],[176,4,178,9]]}
["Factor Entry & Reference",null,null,null,null,"Emission Factor Sources",null,null,null,null,null,null,"Assumptions "]
["Greenhouse Gas Emissions Tracking Spreadsheet",null,null,null,null,"12014 Climate Registry Default Emission Factors in GRP v2.0",null,null,null,null,null,null,"1. Light vehicles were assumed to have average mpg fuel economy (16.7 mpg) unless otherwise specified in Table 1.8 from http://www.eia.gov/totalenergy/data/monthly/#summary."]
["Factor Master List",null,null,null,null,"2http://www.epa.gov/climateleaders/documents/emission-factors.pdf",null,null,null,null,null,null,"2. Heavy vehicles assumed to have average mpg fuel economy (6.2 mpg) unless otherwise specified in Table 1.8 from http://www.eia.gov/totalenergy/data/monthly/#summary."]
[null,null,null,null,null,"3http://epa.gov/fueleconomy/fetrends/1975-2013/420r13011.pdf ",null,null,null,null,null,null,"3. Light vehicles with the same model year are assumed to have the same fuel economy regardless of fuel type."]
[null,null,null,null,null,"4http://www.ghgprotocol.org/files/ghgp/tools/co2-mobile.pdf",null,null,null,null,null,null,"4. Heavy vehicles with the same model year are assumed to have the same fuel economy regardless of fuel type."]
[null,null,null,null,null,"5http://www.eia.gov/emeu/mer/pdf/pages/sec1_17.pdf",null,null,null,null,null,null,"5. Passenger vehicles are assumed to have wheelbase less than or equal to 121 inches."]
[null,null,null,null,null,"6http://www.epa.gov/otaq/nonrdmdl.htm#techrept",null,null,null,null,null,null,"6. Light vehicles not specified as passenger cars are assumed to have wheelbase greater than 121 inches."]
[null,null,null,null,null,"(superscripts indicate emission data source)",null,null,null,null,null,null,"7. Unit Ratios in this tab are calculated based on average vehicle mpg where applicable. Actual conversion factors used may differ from unit ratios based on vehicle mpg entered by user or specified by model year and weight class."]
["Global Warming Potentials (GWPs)"]
["Common Name","Formula","GWP"]
["Carbon dioxide","CO2",1]
["Methane","CH4",21]
["Nitrous Oxide","N2O",310]
["Source: GRP v2.0, April 2014 Table B.1."]
[]
[]
["Electricity"]
["Units\n(Long Name)","Units","Ratio",null,"Emission Factor / eGRID Region","CO2","CH4","N2O","eGRID Subregion Name","Map No."]
[null,null,null,null,null,"lbs/MWh","lbs/MWh","lbs/MWh","Source"]
["Megawatt-Hours","MWh",1,null,"Custom",1041,{"$f":"G35","v":2.8799999999999999E-2},{"$f":"H35","v":2.7789999999999999E-2},"See comment","N/A",null,"Map of U.S. eGRID Subregions, 2004 (from GRP v1.1, May 2008)"]
["Kilowatt-Hours","kWh",{"$f":"1/1000","v":1E-3},null,"NEWE",728.41,{"$f":"75.68/$C$22","v":7.5680000000000011E-2},{"$f":"13.86/$C$22","v":1.3859999999999999E-2},"NPCC New England",1]
["Gigawatt-Hours","GWh",1000,null,"NYCW",610.66999999999996,{"$f":"23.75/$C$22","v":2.375E-2},{"$f":"2.81/$C$22","v":2.81E-3},"NPCC NYC/Westchester",2]
[null,null,null,null,"NYLI",1347.99,{"$f":"96.86/$C$22","v":9.6860000000000002E-2},{"$f":"12.37/$C$22","v":1.2369999999999999E-2},"NPCC Long Island",3]
[null,null,null,null,"NYUP",497.92,{"$f":"15.94/$C$22","v":1.5939999999999999E-2},{"$f":"6.77/$C$22","v":6.77E-3},"NPCC Upstate NY",4]
[null,null,null,null,"RFCE",947.42,{"$f":"26.84/$C$22","v":2.6839999999999999E-2},{"$f":"14.96/$C$22","v":1.4960000000000001E-2},"RFC East",5]
[null,null,null,null,"SRVC",1035.8699999999999,{"$f":"21.15/$C$22","v":2.1149999999999999E-2},{"$f":"17.45/$C$22","v":1.745E-2},"SERC Virginia/Carolina",6]
[null,null,null,null,"SRTV",1357.71,{"$f":"17.28/$C$22","v":1.728E-2},{"$f":"22.09/$C$22","v":2.2089999999999999E-2},"SERC Tennessee Valley",7]
[null,null,null,null,"SRMV",1002.41,{"$f":"19.45/$C$22","v":1.9449999999999999E-2},{"$f":"10.65/$C$22","v":1.065E-2},"SERC Mississippi Valley",8]
[null,null,null,null,"SRSO",1325.68,{"$f":"22.27/$C$22","v":2.2269999999999998E-2},{"$f":"20.78/$C$22","v":2.078E-2},"SERC South",9]
[null,null,null,null,"FRCC",1176.6099999999999,{"$f":"39.24/$C$22","v":3.9240000000000004E-2},{"$f":"13.53/$C$22","v":1.3529999999999999E-2},"FRCC All",10]
[null,null,null,null,"RFCM",1659.46,{"$f":"31.41/$C$22","v":3.141E-2},{"$f":"27.89/$C$22","v":2.7890000000000002E-2},"RFC Michigan",11]
[null,null,null,null,"RFCW",1520.59,{"$f":"18.12/$C$22","v":1.8120000000000001E-2},{"$f":"25.13/$C$22","v":2.513E-2},"RFC West",12]
[null,null,null,null,"MROE",1591.65,{"$f":"23.98/$C$22","v":2.3980000000000001E-2},{"$f":"27.04/$C$22","v":2.7039999999999998E-2},"MRO East",13]
[null,null,null,null,"SRMW",1749.75,{"$f":"19.57/$C$22","v":1.9570000000000001E-2},{"$f":"28.98/$C$22","v":2.8979999999999999E-2},"SERC Midwest",14]
[null,null,null,null,"MROW",1628.6,{"$f":"28.8/$C$22","v":2.8799999999999999E-2},{"$f":"27.79/$C$22","v":2.7789999999999999E-2},"MRO West",15]
[null,null,null,null,"SPNO",1815.76,{"$f":"21.01/$C$22","v":2.1010000000000001E-2},{"$f":"28.89/$C$22","v":2.8889999999999999E-2},"SPP North",16]
[null,null,null,null,"SPSO",1599.02,{"$f":"23.25/$C$22","v":2.325E-2},{"$f":"21.79/$C$22","v":2.179E-2},"SPP South",17]
[null,null,null,null,"ERCT",1181.73,{"$f":"16.7/$C$22","v":1.67E-2},{"$f":"13.1/$C$22","v":1.3099999999999999E-2},"ERCOT All",18]
[null,null,null,null,"RMPA",1824.51,{"$f":"22.25/$C$22","v":2.2249999999999999E-2},{"$f":"27.19/$C$22","v":2.7190000000000002E-2},"WECC Rockies",19]
[null,null,null,null,"AZNM",1191.3499999999999,{"$f":"19.13/$C$22","v":1.9129999999999998E-2},{"$f":"15.58/$C$22","v":1.558E-2},"WECC Southwest",20]
[null,null,null,null,"NWPP",819.21,{"$f":"15.29/$C$22","v":1.529E-2},{"$f":"12.5/$C$22","v":1.2500000000000001E-2},"WECC Northwest",21]
[null,null,null,null,"CAMX",658.68,{"$f":"28.94/$C$22","v":2.894E-2},{"$f":"6.17/$C$22","v":6.1700000000000001E-3},"WECC California",22]
[null,null,null,null,"HIMS",1351.66,{"$f":"72.4/$C$22","v":7.2400000000000006E-2},{"$f":"13.8/$C$22","v":1.3800000000000002E-2},"HICC Miscellaneous",23]
[null,null,null,null,"HIOA",1593.35,{"$f":"101.74/$C$22","v":0.10174},{"$f":"21.98/$C$22","v":2.198E-2},"HICC Oahu",24]
[null,null,null,null,"AKMS",521.26,{"$f":"21.78/$C$22","v":2.1780000000000001E-2},{"$f":"4.28/$C$22","v":4.28E-3},"ASCC Miscellaneous",25]
[null,null,null,null,"AKGD",1280.8599999999999,{"$f":"27.74/$C$22","v":2.7739999999999997E-2},{"$f":"7.69/$C$22","v":7.6900000000000007E-3},"ASCC Alaska Grid",26]
[null,null,null,null,"Source: GRP v2.0, April 2014, Table 14.1. (based on eGrid2012 v1.0, 2009 data) "]
[null,null,null,null,"Xcel Energy Data provided by 2013 Corporate Responsibility Report.  The North States Power Company, Xcel Operations in MN, ND, WI, etc; has a factor of 1,041 lbs/MWh.  Nationwide factor is 1,318 lbs CO2/MWh.  Custom factors for CH4 and N2O are from eGRID map region 15. CH4 and N2O converted to lbs/MWh from lbs/GWh based on 1000MWh/GWh"]
[]
[]
[]
["Natural Gas"]
["Units\n(Long Name)","Units","Ratio",null,"Emission Factor","CO2","CH4","N2O","Notes"]
[null,null,null,null,null,"lbs/scf","lbs/scf","lbs/scf"]
["Cubic foot","cf",1,null,"Default",{"$f":"0.05*2.204","v":0.11020000000000002},{"$f":"0.9/453.6*1028/1000000","v":2.0396825396825396E-6},{"$f":"0.9/453.6*1028/1000000","v":2.0396825396825396E-6}]
["Hundreds of cubic feet","ccf",100,null,"Source: GRP v2.0, April 2014, Table 12.1 (CO2) for \"Unspecified, Weighted US Average\" converted from 0.05 kg/cf to lbs/cf based on 2.204 lbs/kg; and Table 12.5 (CH4, NO2), for \"Boilers\", converted from 0.9 g/MMBtu to lbs/cf based on 453.6 g/lb and 1028 btu/cf (from Table 12.1)."]
["Millions of cubic feet","mmcf",1000000]
["Cubic meters","m3",{"$f":"35.3146667","v":35.314666699999997}]
["Therms","therms",{"$f":"100000/1029","v":97.181729834791057}]
["Millions of Buts","mmbtu",{"$f":"1000000/1029","v":971.81729834791054}]
["Standard Cubic Foot","scf",1]
["Thousand Cubic Feet","mcf",1000]
[]
[]
["Liquefied Petroleum Gas, LPG (Engines)"]
["Units\n(Long Name)","Units","Ratio",null,"Emission Factor","CO2","CH4","N2O","Heating Value (MMBtu/Barrel)",null,"Notes"]
[null,null,null,null,null,"lbs/gal","lbs/gal","lbs/gal"]
["Gallons","Gal",1,null,"Default",{"$f":"5.79*2.204","v":12.76116},{"$f":"0.5/453.6","v":1.1022927689594356E-3},{"$f":"0.22/453.6","v":4.8500881834215163E-4},{"$f":"3.86","v":3.86}]
["Liters","L",{"$f":"1/3.78541178","v":0.26417205263729593},null,"Propane",{"$f":"5.59*2.204","v":12.320360000000001},{"$f":"0.5/453.6","v":1.1022927689594356E-3},{"$f":"0.22/453.6","v":4.8500881834215163E-4},3.82]
[null,null,null,null,"Ethane",{"$f":"4.32*2.204","v":9.5212800000000009},{"$f":"0.5/453.6","v":1.1022927689594356E-3},{"$f":"0.22/453.6","v":4.8500881834215163E-4},2.9]
[null,null,null,null,"Isobutane",{"$f":"6.3*2.204","v":13.885200000000001},{"$f":"0.5/453.6","v":1.1022927689594356E-3},{"$f":"0.22/453.6","v":4.8500881834215163E-4},4.07]
[null,null,null,null,"nButane",{"$f":"6.58*2.204","v":14.502320000000001},{"$f":"0.5/453.6","v":1.1022927689594356E-3},{"$f":"0.22/453.6","v":4.8500881834215163E-4},4.24]
[null,null,null,null,"Source: GRP v2.0, April 2014, Table 13.1 (CO2) for cited petroleum transport fuels (Default = LPG average); all factors converted from their respective kg/gal values to lbs/gal based on 2.204 lbs/kg; and Table 13.7 (CH4, N2O) for \"Other Non-Highway,\" \"Other Small Utility (Gasoline)\", LPG estimated for all fuel types from (Other Small Utility (Gasoline)) and converted from g/gal to lbs/gal based on 453.6 g/lb.  Non-road vehicle factors for LPG fuel were not available. Heating values from Table 13.1."]
[]
[]
[]
[]
["Liquefied Petroleum Gas, LPG (Boilers), including Propane"]
["Units\n(Long Name)","Units","Ratio",null,"Emission Factor","CO2","CH4","N2O","Heating Value (MMBtu/Barrel)",null,"Notes"]
[null,null,null,null,null,"lbs/gal","lbs/gal","lbs/gal"]
["Gallons","Gal",1,null,"Default",{"$f":"5.79*2.204","v":12.76116},{"$f":"0.9*$I$81/42/453.6","v":1.8253968253968252E-4},{"$f":"4*$I$81/42/453.6","v":8.1128747795414452E-4},{"$f":"0.092*C83","v":3.8639999999999999}]
["Liters","L",{"$f":"1/3.78541178","v":0.26417205263729593},null,"Propane",{"$f":"5.74*2.204","v":12.650960000000001},{"$f":"0.9*$I$81/42/453.6","v":1.8253968253968252E-4},{"$f":"4*$I$81/42/453.6","v":8.1128747795414452E-4},{"$f":"0.091*C83","v":3.8220000000000001}]
["Barrels","Barrel",{"$f":"42","v":42},null,"Ethane",{"$f":"4.14*2.204","v":9.1245600000000007},{"$f":"0.9*$I$81/42/453.6","v":1.8253968253968252E-4},{"$f":"4*$I$81/42/453.6","v":8.1128747795414452E-4},{"$f":"0.069*C83","v":2.8980000000000001}]
[null,null,null,null,"Isobutane",{"$f":"6.3*2.204","v":13.885200000000001},{"$f":"0.9*$I$81/42/453.6","v":1.8253968253968252E-4},{"$f":"4*$I$81/42/453.6","v":8.1128747795414452E-4},{"$f":"0.097*C83","v":4.0739999999999998}]
[null,null,null,null,"nButane",{"$f":"6.7*2.204","v":14.766800000000002},{"$f":"0.9*$I$81/42/453.6","v":1.8253968253968252E-4},{"$f":"4*$I$81/42/453.6","v":8.1128747795414452E-4},{"$f":"0.101*C83","v":4.242}]
[null,null,null,null,"Source: GRP v2.0, April 2014, Table 12.1 (CO2) for cited petroleum product (Default = LPG average); all factors converted from their respective kg/gal values to lbs/gal based on 2.204 lbs/kg; and Table 12.7 (CH4, N2O) for \"Liquefied Petroleum Gases Boilers), converted from respective g/MMBtu values to lbs/gal based on heating values from Table 12.1, 453.6 grams/lb, and 42 gallons/barrel (barrel conversion factor from GRP 2.0 Appendix C). Heating values from Table 12.1. Boiler values of CH4 and N2O for specific LPG fuels not available so assumed all fuel types have same CH4 and N2O emissions in Boilers as LPG average."]
[]
[]
[]
[]
[]
["Diesel (Internal Combustion Engines, Non-Highway)"]
["Units\n(Long Name)","Units","Ratio",null,"Emission Factor","CO2","CH4","N2O","Notes"]
[null,null,null,null,null,"lbs/gal","lbs/gal","lbs/gal"]
["Gallons","Gal",1,null,"Default",{"$f":"10.21*2.204","v":22.502840000000003},{"$f":"0.58/453.6","v":1.2786596119929452E-3},{"$f":"0.26/453.6","v":5.7319223985890654E-4},"Tier B/C Method"]
["Liters","L",{"$f":"1/3.78541178","v":0.26417205263729593},null,"Source: GRP v2.0, April 2014, Table 13.1 (CO2) for \"Diesel Fuel No 1 and 2\" converted from  kg/gal to lbs/gal based on 2.204 lbs/kg; and Table 13.7 (CH4, NO2), for \"Other Non-Highway\", converted from respective g/gal values to lbs/gal based on 453.6 g/lb."]
[]
[]
[]
["Gasoline (Internal Combustion Engines, Non-Highway)"]
["Units\n(Long Name)","Units","Ratio",null,"Emission Factor","CO2","CH4","N2O","Notes"]
[null,null,null,null,null,"lbs/gal","lbs/gal","lbs/gal"]
["Gallons","Gal",1,null,"Default",{"$f":"8.78*2.204","v":19.351120000000002},{"$f":"0.5/453.6","v":1.1022927689594356E-3},{"$f":"0.22/453.6","v":4.8500881834215163E-4},"Tier B/C Method"]
["Liters","L",{"$f":"1/3.78541178","v":0.26417205263729593},null,"Source: GRP v2.0, April 2014, Table 13.1 (CO2) for \"Motor Gasoline\" converted from  kg/gal to lbs/gal based on 2.204 lbs/kg; and Table 13.7 (CH4, NO2), for \"Other Non-Highway\", converted from respective g/gal values to lbs/gal based on 453.6 g/lb."]
[]
[]
[]
["Refrigerants"]
["Units\n(Long Name)","Units","Ratio",null,"Emission Factor","CO2","CH4","N2O","Notes"]
[null,null,null,null,null,"(unitless)","(unitless)","(unitless)"]
["Pounds","lb",1,null,"HFC-23",11700,0,0,"GWP, in CO2-e, unitless (i.e. lb/lb refrigerant)"]
["Grams","g",{"$f":"1/453.6","v":2.2045855379188711E-3},null,"HFC-32",650,0,0,"GWP, in CO2-e, unitless (i.e. lb/lb refrigerant)"]
["Kilogram","kg",2.2040000000000002,null,"HFC-125",2800,0,0,"GWP, in CO2-e, unitless (i.e. lb/lb refrigerant)"]
[null,null,null,null,"HFC-134a",1300,0,0,"GWP, in CO2-e, unitless (i.e. lb/lb refrigerant)"]
[null,null,null,null,"HFC-143a",3800,0,0,"GWP, in CO2-e, unitless (i.e. lb/lb refrigerant)"]
[null,null,null,null,"HFC-152a",140,0,0,"GWP, in CO2-e, unitless (i.e. lb/lb refrigerant)"]
[null,null,null,null,"HFC-227ea",2900,0,0,"GWP, in CO2-e, unitless (i.e. lb/lb refrigerant)"]
[null,null,null,null,"HFC-236fa",6300,0,0,"GWP, in CO2-e, unitless (i.e. lb/lb refrigerant)"]
[null,null,null,null,"R-410A",1725,0,0,"GWP, in CO2-e, unitless (i.e. lb/lb refrigerant)"]
[null,null,null,null,"PFC-116",9200,0,0,"GWP, in CO2-e, unitless (i.e. lb/lb refrigerant)"]
[null,null,null,null,"PFC-14",6500,0,0,"GWP, in CO2-e, unitless (i.e. lb/lb refrigerant)"]
[null,null,null,null,"PFC-410",7000,0,0,"GWP, in CO2-e, unitless (i.e. lb/lb refrigerant)"]
[null,null,null,null,"Source: GRP v2.0, April 2014, Table B.1 except PFC-410.  PFC-410 GWP from http://www.epa.gov/climateleaders/documents/resources/mfgrfg.pdf. Factors are global warming potentials, in terms of CO2 equivalents."]
[]
[]
[]
["Welding (Acetylene)"]
["Units\n(Long Name)","Units","Ratio",null,"Emission Factor","CO2","CH4","N2O","Notes"]
[null,null,null,null,null,"lbs/lb","lbs/lb","lbs/lb"]
["Pounds","lb",1,null,"Default",{"$f":"C130*0.1053*2.20462/C132","v":1.5792277959183674E-2},0,0,"Assuming 100% oxidation, no CH4 or N2O"]
["Kilogram","kg",2.2040000000000002,null,"Source: GRP v2.0, April 2014, Table 12.1 and http://www.oregon.gov/osp/SFM/docs/cr2k/cr2k_general/gasconversionchartpublic.pdf ; Converted to lbs/lb based on 14.70 lbs/scf, 0.1053 kg CO2/scf, and 2.20462 lbs/kg"]
["Cubic Feet","cf",{"$f":"C130*14.7","v":14.7}]
["Cubic meters","m3",{"$f":"C132*35.315","v":519.13049999999998}]
[]
[]
["Gasoline (Light Trucks), including all Gasoline-Ethanol Blends"]
["Units\n(Long Name)","Units","Ratio",null,"Emission Factor","CO2","CH4","N2O","Notes"]
[null,null,null,null,null,"lbs/gal","lbs/gal","lbs/gal"]
["Gallons","Gal",1,null,"Default",{"$f":"8.78*2.204","v":19.351120000000002},{"$f":"(0.0178/453.6)*16","v":6.2786596119929455E-4},{"$f":"(0.0228/453.6)*16","v":8.0423280423280426E-4},"Tier B/C Method (CO2)"]
["Liters","L",{"$f":"1/3.78541178","v":0.26417205263729593},null,"Source: GRP v2.0, April 2014, Table 13.1 (CO2) for \"Gasoline\" converted from  kg/gal to lbs/gal based on 2.204 lbs/kg; Table 13.5 (CH4, N2O) calculated based on 0.0178 g/mi and 0.0228 g/mi, respectively, for \"Gasoline Light Trucks for Model Year 2002,\" an average of 16 miles per gallon and 453.6 g/lb."]
[]
[]
[]
[]
["Diesel (Automobiles)"]
["Units\n(Long Name)","Units","Ratio",null,"Emission Factor","CO2","CH4","N2O","Notes"]
[null,null,null,null,null,"lbs/gal","lbs/gal","lbs/gal"]
["Gallons","Gal",1,null,"Default",{"$f":"10.21*2.204","v":22.502840000000003},{"$f":"(0.001/453.6)*16","v":3.5273368606701937E-5},{"$f":"(0.0015/453.6)*16","v":5.2910052910052905E-5},"Tier B/C Method (CO2)"]
["Liters","L",{"$f":"1/3.78541178","v":0.26417205263729593},null,"Source: GRP v2.0, April 2014, Table 13.1 (CO2) for \"Diesel Fuel No 1 and 2\" converted from  kg/gal to lbs/gal based on 2.204 lbs/kg; Table 13.5 (CH4, N2O) calculated based on 0.0010 g/mi and 0.0015 g/mi, respectively, for \"Diesel Light Trucks Model Years 1996-2011\", an average of 16 miles per gallon  and 453.6 g/lb."]
[]
[]
[]
[]
["Ethanol, 100% Only (Automobiles)"]
["Units\n(Long Name)","Units","Ratio",null,"Emission Factor","CO2","CH4","N2O","Notes"]
[null,null,null,null,null,"lbs/gal","lbs/gal","lbs/gal"]
["Gallons","Gal",1,null,"Default",{"$f":"5.75*2.204","v":12.673000000000002},{"$f":"(0.055/453.6)*16","v":1.9400352733686065E-3},{"$f":"(0.067/453.6)*16","v":2.3633156966490301E-3},"Tier B/C Method"]
["Liters","L",{"$f":"1/3.78541178","v":0.26417205263729593},null,"Source: GRP v2.0, April 2014, Table 13.1 (CO2) for \"Ethanol (E100)\" converted from  kg/gal to lbs/gal based on 2.204 lbs/kg; Table 13.6 (CH4, N2O) calculated based on 0.055 g/mi and 0.067 g/mi, respectively, for \"Light Duty Vehicles, Ethanol\", an average of 16 miles per gallon 453.6 g/lb."]
[]
[]
[]
[]
["Vehicles (Automobiles, Light Trucks)"]
["Units\n(Long Name)","Units","Ratio",null,"Emission Factor","CO2","CH4","N2O","Notes"]
[null,null,null,null,null,"lbs/gal","lbs/gal","lbs/gal"]
["Gallons","Gal",1,null,"Gasoline",{"$f":"F139","v":19.351120000000002},{"$f":"G139","v":6.2786596119929455E-4},{"$f":"H139","v":8.0423280423280426E-4},"Tier B/C Method"]
["Liters","L",{"$f":"1/3.78541178","v":0.26417205263729593},null,"Diesel",{"$f":"F148","v":22.502840000000003},{"$f":"G148","v":3.5273368606701937E-5},{"$f":"H148","v":5.2910052910052905E-5},"Tier B/C Method"]
[null,null,null,null,"E100",{"$f":"F157","v":12.673000000000002},{"$f":"G157","v":1.9400352733686065E-3},{"$f":"H157","v":2.3633156966490301E-3},"Tier B/C Method"]
[null,null,null,null,"E85",{"$f":"(F$166*0.15 + F$168 *0.85)","v":13.674718000000002},{"$f":"(G$166*0.15 + G$168 *0.85)","v":1.7432098765432097E-3},{"$f":"(H$166*0.15 + H$168 *0.85)","v":2.1294532627865962E-3},"Tier B/C Method"]
[null,null,null,null,"E15",{"$f":"(F$166*0.85 + F$168 *0.15)","v":18.349402000000001},{"$f":"(G$166*0.85 + G$168 *0.15)","v":8.2469135802469128E-4},{"$f":"(H$166*0.85 + H$168 *0.15)","v":1.0380952380952381E-3},"Tier B/C Method"]
[null,null,null,null,"E12",{"$f":"(F$166*0.88 + F$168 *0.12)","v":18.549745600000001},{"$f":"(G$166*0.88 + G$168 *0.12)","v":7.8532627865961202E-4},{"$f":"(H$166*0.88 + H$168 *0.12)","v":9.913227513227514E-4},"Tier B/C Method"]
[null,null,null,null,"E10",{"$f":"(F$166*0.9 + F$168 *0.1)","v":18.683308},{"$f":"(G$166*0.9 + G$168 *0.1)","v":7.5908289241622578E-4},{"$f":"(H$166*0.9 + H$168 *0.1)","v":9.6014109347442684E-4},"Tier B/C Method"]
[null,null,null,null,"E5",{"$f":"(F$166*0.95 + F$168 *0.05)","v":19.017213999999999},{"$f":"(G$166*0.95 + G$168 *0.05)","v":6.9347442680776016E-4},{"$f":"(H$166*0.95 + H$168 *0.05)","v":8.8218694885361555E-4},"Tier B/C Method"]
[null,null,null,null,"Biodiesel",{"$f":"9.45*2.204","v":20.8278},{"$f":"(0.055/453.6)*14","v":1.6975308641975306E-3},{"$f":"(0.067/453.6)*14","v":2.0679012345679012E-3},"Tier B/C Method"]
[]
[]
[null,null,null,null,"Source: GRP v2.0, April 2014, Table 13.1 (CO2) converted from  kg/gal to lbs/gal based on 2.204 lbs/kg; Table 13.5 (CH4, N2O) for ethanol calculated based on 0.055 g/mi and 0.067 g/mi, respectively, for \"Light Duty Vehicles, Ethanol\", an average of 14 miles per gallon, 453.6 g/lb. Ethanol blends emissions calculated as weighted average of percent ethanol to percent gasoline. "]
[]
[]
[]
["Composting Factors"]
["Types of Systems",null,null,null,"Emission Factor","CO2","CH4","N2O","Notes"]
[null,null,null,null,null,"tCO2e/MT","tCO2e/MT","tCO2e/MT"]
["Turned System - No Cover",null,null,null,null,0,0.09,0.09]
["Turned System - Covered",null,null,null,null,0,0.06,0.09]
["Forced Aeration System - No Optional Process Controls",null,null,null,null,0,0.06,0.06]
["Forced Aeration System - ASP with Synthetic Cover",null,null,null,null,0,0.03,0.06]
["Forced Aeration System - Positive Aeration",null,null,null,null,0,0.03,0.06]
["Forced Aeration System - Negative Aeration",null,null,null,null,0,0.03,0.06]
[null,null,null,null,"Source: Climate Action Reserve Organic Waste Composting Project Protocol Version 1.1, July 2013"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Landfill Gas Calculator"]
[null,"Default","User Defined"]
["% CH4",0.5,0.5]
["Destruction Efficiency",0.99,0.99]
["Collection Efficiency",0.75,0.75]
["Oxidation Factor",0.1,0.1]
["Unit Conversion (volume to mass)",19.125,19.125]
["GWP",21,21]
["Source: Local Government Operations Protocol Version 1.1, May 2010"]
[]
[]
[]
[]
[]
[]
["Compressed Natural Gas Vehicles"]
["Units\n(Long Name)","Units","Ratio",null,"Emission Factor","Year","CO2","CH4","N2O"]
[null,null,null,null,null,null,"lbs/scf","g/mile","g/mile"]
["Mile","miles",1,null,"2Compressed Natural Gas (CNG)-light","N/A",{"$f":"0.0545/2.204","v":2.4727767695099816E-2},0.73699999999999999,0.05]
["Cubic foot","scf",{"$f":"16*7.48","v":119.68},null,"2Compressed Natural Gas (CNG)-heavy","N/A",{"$f":"0.0545/2.204","v":2.4727767695099816E-2},1.966,0.17499999999999999]
["Hundreds of cubic feet","ccf",{"$f":"C219*100","v":11968},null,"Source: 2http://www.epa.gov/climateleaders/documents/emission-factors.pdf       "]
["Millions of cubic feet","mmcf",{"$f":"C219*10^6","v":119680000}]
["Cubic meters","m3",{"$f":"C219*35.3146667","v":4226.4593106559996}]
["Therms","therms",{"$f":"C219*100000/1029","v":11630.709426627795}]
["Millions of Btus","mmbtu",{"$f":"C219*1000000/1029","v":116307.09426627794}]
["Thousand Cubic Feet","mcf",{"$f":"C219*1000","v":119680}]
[]
[]
["Gasoline (Light Trucks)"]
["Units\n(Long Name)","Units","Ratio",null,"Emission Factor","Year","CO22,3","CH42","N2O2"]
[null,null,null,null,null,null,"g/mile","g/mile","g/mile"]
["Miles","Miles",1,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",1983,504,0.1368,7.22E-2]
["Gallons","Gal",{"$f":"16","v":16},null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",1984,512,0.12939999999999999,7.6399999999999996E-2]
["Liters","L",{"$f":"(16)/3.78541178","v":4.2267528421967349},null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",1985,509,0.122,8.0600000000000005E-2]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",1986,489,0.11459999999999999,8.48E-2]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",1987,486,8.1299999999999997E-2,0.10349999999999999]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",1988,498,8.1299999999999997E-2,0.10349999999999999]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",1989,506,8.1299999999999997E-2,0.10349999999999999]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",1990,512,8.1299999999999997E-2,0.10349999999999999]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",1991,500,8.1299999999999997E-2,0.10349999999999999]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",1992,512,8.1299999999999997E-2,0.10349999999999999]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",1993,507,8.1299999999999997E-2,0.10349999999999999]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",1994,518,6.4600000000000005E-2,9.8199999999999996E-2]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",1995,524,5.1700000000000003E-2,9.0800000000000006E-2]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",1996,518,4.5199999999999997E-2,8.7099999999999997E-2]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",1997,528,4.5199999999999997E-2,8.7099999999999997E-2]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",1998,521,3.9100000000000003E-2,7.2800000000000004E-2]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",1999,535,3.2099999999999997E-2,5.6399999999999999E-2]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",2000,528,3.4599999999999999E-2,6.2100000000000002E-2]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",2001,538,1.5100000000000001E-2,1.6400000000000001E-2]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",2002,539,1.78E-2,2.2800000000000001E-2]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",2003,533,1.55E-2,1.14E-2]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",2004,538,1.52E-2,1.32E-2]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",2005,526,1.5699999999999999E-2,1.01E-2]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",2006,518,1.5900000000000001E-2,8.8999999999999999E-3]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",2007,512,1.61E-2,7.9000000000000008E-3]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",2008,499,1.6299999999999999E-2,6.6E-3]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",2009,480,1.6299999999999999E-2,6.6E-3]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",2010,474,1.6299999999999999E-2,6.6E-3]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",2011,466,1.6299999999999999E-2,6.6E-3]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",2012,461,1.6299999999999999E-2,6.6E-3]
[null,null,null,null,"Gasoline Light-duty Trucks (Vans, Pickups, Trucks, SUVs)",2013,452,1.6299999999999999E-2,6.6E-3]
[null,null,null,null,"Source: 2http://www.epa.gov/climateleaders/documents/emission-factors.pdf ; 3http://epa.gov/fueleconomy/fetrends/1975-2013/420r13011.pdf       "]
[]
[]
["Gasoline (Heavy Trucks)"]
["Units\n(Long Name)","Units","Ratio",null,"Emission Factor","Year","CO2","CH4","N2O"]
["Miles","Miles",1,null,null,null,"lbs/mile","g/mile","g/mile"]
["Gallons","Gal",{"$f":"6","v":6},null,"Gasoline Heavy-duty Vehicles","<1981",null,0.46039999999999998,4.9700000000000001E-2]
["Liters","L",{"$f":"(6)/3.78541178","v":1.5850323158237754},null,"Gasoline Heavy-duty Vehicles","1982-84",null,0.44919999999999999,5.3800000000000001E-2]
[null,null,null,null,"Gasoline Heavy-duty Vehicles","1985-86",null,0.40899999999999997,5.1499999999999997E-2]
[null,null,null,null,"Gasoline Heavy-duty Vehicles",1987,null,0.36749999999999999,8.4900000000000003E-2]
[null,null,null,null,"Gasoline Heavy-duty Vehicles","1988-1989",null,0.34920000000000001,9.3299999999999994E-2]
[null,null,null,null,"Gasoline Heavy-duty Vehicles","1990-1995",null,0.3246,0.1142]
[null,null,null,null,"Gasoline Heavy-duty Vehicles",1996,null,0.1278,0.16800000000000001]
[null,null,null,null,"Gasoline Heavy-duty Vehicles",1997,null,9.2399999999999996E-2,0.1726]
[null,null,null,null,"Gasoline Heavy-duty Vehicles",1998,null,6.4100000000000004E-2,0.16930000000000001]
[null,null,null,null,"Gasoline Heavy-duty Vehicles",1999,null,5.7799999999999997E-2,0.14349999999999999]
[null,null,null,null,"Gasoline Heavy-duty Vehicles",2000,null,4.9299999999999997E-2,0.10920000000000001]
[null,null,null,null,"Gasoline Heavy-duty Vehicles",2001,null,5.28E-2,0.1235]
[null,null,null,null,"Gasoline Heavy-duty Vehicles",2002,null,5.4600000000000003E-2,0.13070000000000001]
[null,null,null,null,"Gasoline Heavy-duty Vehicles",2003,null,5.33E-2,0.124]
[null,null,null,null,"Gasoline Heavy-duty Vehicles",2004,null,3.4099999999999998E-2,2.8500000000000001E-2]
[null,null,null,null,"Gasoline Heavy-duty Vehicles",2005,null,3.2599999999999997E-2,1.77E-2]
[null,null,null,null,"Gasoline Heavy-duty Vehicles",2006,null,3.27E-2,1.7100000000000001E-2]
[null,null,null,null,"Gasoline Heavy-duty Vehicles",2007,null,3.3000000000000002E-2,1.5299999999999999E-2]
[null,null,null,null,"Gasoline Heavy-duty Vehicles","2008-present",null,3.3300000000000003E-2,1.34E-2]
[null,null,null,null,"Source: 2http://www.epa.gov/climateleaders/documents/emission-factors.pdf ; CO2 emission factors from Heavy Automobiles Table below."]
[]
[]
["Gasoline Light Passenger Cars"]
["Units\n(Long Name)","Units","Ratio",null,"Emission Factor","Year","CO22,3","CH42","N2O2"]
["Miles","Miles",1,null,null,null,"g/mile","g/mile","g/mile"]
["Gallons","Gal",{"$f":"16","v":16},null,"Gasoline Passenger Cars",1983,{"$f":"403","v":403},7.8200000000000006E-2,6.3E-2]
["Liters","L",{"$f":"(16)/3.78541178","v":4.2267528421967349},null,"Gasoline Passenger Cars",1984,{"$f":"397","v":397},7.0400000000000004E-2,6.4699999999999994E-2]
[null,null,null,null,"Gasoline Passenger Cars",1985,{"$f":"387","v":387},7.0400000000000004E-2,6.4699999999999994E-2]
[null,null,null,null,"Gasoline Passenger Cars",1986,{"$f":"375","v":375},7.0400000000000004E-2,6.4699999999999994E-2]
[null,null,null,null,"Gasoline Passenger Cars",1987,374,7.0400000000000004E-2,6.4699999999999994E-2]
[null,null,null,null,"Gasoline Passenger Cars",1988,369,7.0400000000000004E-2,6.4699999999999994E-2]
[null,null,null,null,"Gasoline Passenger Cars",1989,376,7.0400000000000004E-2,6.4699999999999994E-2]
[null,null,null,null,"Gasoline Passenger Cars",1990,382,7.0400000000000004E-2,6.4699999999999994E-2]
[null,null,null,null,"Gasoline Passenger Cars",1991,382,7.0400000000000004E-2,6.4699999999999994E-2]
[null,null,null,null,"Gasoline Passenger Cars",1992,389,7.0400000000000004E-2,6.4699999999999994E-2]
[null,null,null,null,"Gasoline Passenger Cars",1993,386,7.0400000000000004E-2,6.4699999999999994E-2]
[null,null,null,null,"Gasoline Passenger Cars",1994,386,5.3100000000000001E-2,5.6000000000000001E-2]
[null,null,null,null,"Gasoline Passenger Cars",1995,382,3.5799999999999998E-2,4.7300000000000002E-2]
[null,null,null,null,"Gasoline Passenger Cars",1996,384,2.7199999999999998E-2,4.2599999999999999E-2]
[null,null,null,null,"Gasoline Passenger Cars",1997,384,2.6800000000000001E-2,4.2200000000000001E-2]
[null,null,null,null,"Gasoline Passenger Cars",1998,386,2.4899999999999999E-2,3.9300000000000002E-2]
[null,null,null,null,"Gasoline Passenger Cars",1999,392,2.1600000000000001E-2,3.3700000000000001E-2]
[null,null,null,null,"Gasoline Passenger Cars",2000,395,1.78E-2,2.7300000000000001E-2]
[null,null,null,null,"Gasoline Passenger Cars",2001,393,1.0999999999999999E-2,1.5800000000000002E-2]
[null,null,null,null,"Gasoline Passenger Cars",2002,390,1.0699999999999999E-2,1.5299999999999999E-2]
[null,null,null,null,"Gasoline Passenger Cars",2003,386,1.14E-2,1.35E-2]
[null,null,null,null,"Gasoline Passenger Cars",2004,389,1.4500000000000001E-2,8.3000000000000001E-3]
[null,null,null,null,"Gasoline Passenger Cars",2005,384,1.47E-2,7.9000000000000008E-3]
[null,null,null,null,"Gasoline Passenger Cars",2006,386,1.61E-2,5.7000000000000002E-3]
[null,null,null,null,"Gasoline Passenger Cars",2007,375,1.7000000000000001E-2,4.1000000000000003E-3]
[null,null,null,null,"Gasoline Passenger Cars",2008,372,1.72E-2,3.8E-3]
[null,null,null,null,"Gasoline Passenger Cars",2009,356,1.7299999999999999E-2,3.5999999999999999E-3]
[null,null,null,null,"Gasoline Passenger Cars",2010,346,1.7299999999999999E-2,3.5999999999999999E-3]
[null,null,null,null,"Gasoline Passenger Cars",2011,348,1.7299999999999999E-2,3.5999999999999999E-3]
[null,null,null,null,"Gasoline Passenger Cars",2012,329,1.7299999999999999E-2,3.5999999999999999E-3]
[null,null,null,null,"Gasoline Passenger Cars",2013,325,1.7299999999999999E-2,3.5999999999999999E-3]
[null,null,null,null,"Source: 2http://www.epa.gov/climateleaders/documents/emission-factors.pdf ; 3http://epa.gov/fueleconomy/fetrends/1975-2013/420r13011.pdf       "]
[]
[]
["Diesel Vehicles"]
["Units\n(Long Name)","Units","Ratio",null,"Emission Factor","Year","CO2","CH4","N2O"]
["Miles","Miles",1,null,null,null,"lbs/mile","g/mile","g/mile"]
["Gallons","Gal",{"$f":"7","v":7},null,"Diesel Medium and Heavy-Duty Vehicles","1960-present",null,5.1000000000000004E-3,4.7999999999999996E-3]
["Liters","L",{"$f":"(7)/3.78541178","v":1.8492043684610713},null,"Diesel Light-Duty Trucks","1960-1982",null,5.9999999999999995E-4,1.1999999999999999E-3]
[null,null,null,null,"Diesel Light-Duty Trucks","1983-1995",null,5.0000000000000001E-4,1E-3]
[null,null,null,null,"Diesel Light-Duty Trucks","1996-present",null,5.0000000000000001E-4,1E-3]
[null,null,null,null,"Diesel Passenger Cars ","1960-1982",null,1.1000000000000001E-3,1.6999999999999999E-3]
[null,null,null,null,"Diesel Passenger Cars ","1983-1995",null,8.9999999999999998E-4,1.4E-3]
[null,null,null,null,"Diesel Passenger Cars ","1996-present",null,1E-3,1.5E-3]
[null,null,null,null,"Passenger Car","N/A",0.36799999999999999,1.7999999999999999E-2,1.2999999999999999E-2]
[null,null,null,null,"Source: 2http://www.epa.gov/climateleaders/documents/emission-factors.pdf ; CO2 emission factors for Heavy Vehicles can be found in the table below."]
[]
[]
[]
["Heavy Automobiles"]
["Units\n(Long Name)","Units","Ratio",null,"Emission Factor","Year","CO2","Estimated MPG"]
["Gallons","Gal",1,null,null,null,"lbs/km"]
["Liters","L",{"$f":"1/3.78541178","v":0.26417205263729593},null,"Diesel heavy truck","N/A",0.87,"7 mpg"]
[null,null,null,null,"Gasoline heavy truck","N/A",0.92400000000000004,"6 mpg"]
[null,null,null,null,"Source: 4http://www.ghgprotocol.org/files/ghgp/tools/co2-mobile.pdf"]
[]
[]
[]
[]
[]
[]
[]
["Table 1.8:"]
["Year","Light-Duty  Vehicles, Short Wheelbasea","Light-Duty  Vehicles, Long Wheelbaseb",null,"Heavy-Duty Trucksc","All Motor Vehiclesd"]
[null,"Fuel Economy","Fuel Economy",null,"Fuel Economy","Fuel Economy"]
[null,"Miles per Gallon","Miles per Gallon",null,"Miles per Gallon","Miles per Gallon"]
["1980 ..........",16,12.2,null,5.4,13.3]
["1985 ..........",17.5,14.3,null,5.8,14.6]
["1990 ..........",20.2,16.100000000000001,null,6,16.399999999999999]
["1995 ..........",21.1,17.3,null,6.1,16.8]
["2000 ..........",21.9,17.399999999999999,null,5.8,16.899999999999999]
["2001 ..........",22.1,17.600000000000001,null,5.9,17.100000000000001]
["2002 ..........",22,17.5,null,5.8,16.899999999999999]
["2003 ..........",22.2,16.2,null,6.7,17]
["2004 ..........",22.5,16.2,null,6.7,17.100000000000001]
["2005 ..........",22.1,17.7,null,6,17.100000000000001]
["2006 ..........",22.5,17.8,null,5.9,17.2]
["2007 ..........","22.9a ","17.1b ",null,6.4,17.2]
["2008 ..........",23.7,17.3,null,6.5,17.399999999999999]
["2009 ..........",23.5,17.3,null,6.5,17.600000000000001]
["2010 ..........",23.3,17.2,null,6.4,17.399999999999999]
["2011 ..........",23.2,17.100000000000001,null,6.3,17.5]
["2012P  .......",23.3,17.100000000000001,null,6.4,17.600000000000001]
["Average",{"$f":"(SUM(B359:B369)+22.9+SUM(B371:B375))/17","v":21.764705882352942},{"$f":"(SUM(C359:C369)+17.1+SUM(C371:C375))/17","v":16.670588235294115},{"$f":"(SUM(D359:D369)+22.9+SUM(D371:D375))/17","v":1.3470588235294116},{"$f":"AVERAGE(E359:E375)","v":6.1529411764705895},{"$f":"AVERAGE(F359:F375)","v":16.77058823529412}]
["Web Page:  http://www.eia.gov/totalenergy/data/monthly/#summary."]
["5Source:  Table 1.8. http://www.eia.gov/totalenergy/data/monthly/#summary."]
["a Through 1989, data are for passenger cars and motorcycles. For 1990–2006, data are for passenger cars only. Beginning in 2007, data are for light-duty vehicles (passenger cars, light trucks, vans, and sport utility vehicles) with a wheelbase less than or equal to 121 inches."]
["b For 1966–2006, data are for vans, pickup trucks, and sport utility vehicles. Beginning in 2007, data are for light-duty vehicles (passenger cars, light trucks, vans, and sport utility vehicles) with a wheelbase greater than 121 inches."]
["c For 1949–1965, data are for single-unit trucks with 2 axles and 6 or more tires, combination trucks, and other vehicles with  2 axles and 4  tires that are not passenger cars. For 1965–2006, data are for single-unit trucks with 2 axles and 6 or more tires, and combination trucks. Beginning in 2007, data are for single-unit trucks with 2 axles and 6 or more tires (or a gross vehicle weight rating exceeding 10,000 pounds), and combination trucks."]
["d Includes buses and motorcycles, which are not separately displayed."]
["P=Preliminary."]
["Web Page: See http://www.eia.gov/totalenergy/data/monthly/#summary (Excel and CSV files) for all available annual data beginning in 1949."]
["Sources:  Light-Duty Vehicles, Short Wheelbase: 1990–1994—U.S. Department of Transportation, Bureau of Transportation Statistics, National Transportation Statistics 1998, Table 4-13.  All Other Data: 1949–1994—Federal Highway Administration (FHWA), Highway Statistics Summary to 1995, Table VM-201A. 1995 forward—FHWA, Highway Statistics, annual reports, Table VM-1."]
["U.S. Energy Information Administration / Monthly Energy Review October 2014 / 40th Anniversary Issue                    17"]
[]
[]
[]
[]
[]
["Off-Road Compression Ignition: Diesel"]
["Units\n(Long Name)","Units","Ratio",null,"Horse Power (hp)","Tier","BSFC (lb/hp*hr)","HC","CO2"]
["Gallons","Gal",1,null,null,null,null,"(g/hp*hr)","(g/gal)"]
["Liters","L",{"$f":"1/3.78541178","v":0.26417205263729593},null,"0 to 11","Tier 0",0.40799999999999997,1.5,{"$f":"(G395*453.6-H395)*0.87*(44/12)","v":585.58447200000001}]
[null,null,null,null,null,"Tier 1",0.40799999999999997,0.76280000000000003,{"$f":"(G396*453.6-H396)*0.87*(44/12)","v":587.93614000000002}]
[null,null,null,null,null,"Tier 2",0.40799999999999997,0.55079999999999996,588.61242000000004]
[null,null,null,null,null,"Tier 4",0.40799999999999997,0.55079999999999996,588.61242000000004]
[null,null,null,null,"11 to 25","Tier 0",0.40799999999999997,1.7,584.94647200000009]
[null,null,null,null,null,"Tier 1",0.40799999999999997,0.438,588.97225200000003]
[null,null,null,null,null,"Tier 2",0.40799999999999997,0.438,588.97225200000003]
[null,null,null,null,null,"Tier 4",0.40799999999999997,0.438,588.97225200000003]
[null,null,null,null,"25 to 50","Tier 0",0.40799999999999997,1.8,584.62747200000001]
[null,null,null,null,null,"Tier 1",0.40799999999999997,0.27889999999999998,589.47978100000012]
[null,null,null,null,null,"Tier 2",0.40799999999999997,0.27889999999999998,589.47978100000012]
[null,null,null,null,null,"Tier 4",0.40799999999999997,0.13139999999999999,589.95030599999996]
[null,null,null,null,"50 to 75","Tier 0",0.40799999999999997,0.99,587.21137199999998]
[null,null,null,null,null,"Tier 1",0.40799999999999997,0.52129999999999999,588.70652500000006]
[null,null,null,null,null,"Tier 2",0.40799999999999997,0.36720000000000003,589.19810399999994]
[null,null,null,null,null,"Tier 4",0.40799999999999997,0.13139999999999999,589.95030599999996]
[null,null,null,null,"75 to 100","Tier 0",0.40799999999999997,0.99,587.21137199999998]
[null,null,null,null,null,"Tier 1",0.40799999999999997,0.52129999999999999,588.70652500000006]
[null,null,null,null,null,"Tier 2",0.40799999999999997,0.36720000000000003,589.19810399999994]
[null,null,null,null,null,"Tier 3",0.40799999999999997,0.18360000000000001,589.78378799999996]
[null,null,null,null,null,"Tier 4",0.40799999999999997,0.13139999999999999,589.95030599999996]
[null,null,null,null,"100 to 175","Tier 0",0.36699999999999999,{"$f":"0.68","v":0.68},528.87392799999998]
[null,null,null,null,null,"Tier 1",0.36699999999999999,{"$f":"0.3384","v":0.33839999999999998},529.96363199999996]
[null,null,null,null,null,"Tier 2",0.36699999999999999,{"$f":"0.3384","v":0.33839999999999998},529.96363199999996]
[null,null,null,null,null,"Tier 3",0.36699999999999999,{"$f":"0.1836","v":0.18360000000000001},530.4574439999999]
[null,null,null,null,null,"Tier 4",0.36699999999999999,{"$f":"0.1314","v":0.13139999999999999},530.62396199999989]
[null,null,null,null,"175 to 300","Tier 0",0.36699999999999999,0.68,528.87392799999998]
[null,null,null,null,null,"Tier 1",0.36699999999999999,0.3085,530.05901300000005]
[null,null,null,null,null,"Tier 2",0.36699999999999999,0.3085,530.05901300000005]
[null,null,null,null,null,"Tier 3",0.36699999999999999,0.18360000000000001,530.4574439999999]
[null,null,null,null,null,"Tier 4",0.36699999999999999,0.13139999999999999,530.62396199999989]
[null,null,null,null,"300 to 600","Tier 0",0.36699999999999999,0.68,528.87392799999998]
[null,null,null,null,null,"Tier 1",0.36699999999999999,0.20250000000000001,530.397153]
[null,null,null,null,null,"Tier 2",0.36699999999999999,0.16689999999999999,530.510717]
[null,null,null,null,null,"Tier 3",0.36699999999999999,0.16689999999999999,530.510717]
[null,null,null,null,null,"Tier 4",0.36699999999999999,0.13139999999999999,530.62396199999989]
[null,null,null,null,"600 to 750","Tier 0",0.36699999999999999,0.68,528.87392799999998]
[null,null,null,null,null,"Tier 1",0.36699999999999999,0.14729999999999999,530.57324100000005]
[null,null,null,null,null,"Tier 2",0.36699999999999999,0.16689999999999999,530.510717]
[null,null,null,null,null,"Tier 3",0.36699999999999999,0.16689999999999999,530.510717]
[null,null,null,null,null,"Tier 4",0.36699999999999999,0.13139999999999999,530.62396199999989]
[null,null,null,null,">750","Tier 0",0.36699999999999999,0.68,528.87392799999998]
[null,null,null,null,null,"Tier 1",0.36699999999999999,0.28610000000000002,530.13046900000006]
[null,null,null,null,null,"Tier 2",0.36699999999999999,0.16689999999999999,530.510717]
[null,null,null,null,null,"Tier 4",0.36699999999999999,0.28149999999999997,530.14514300000008]
[null,null,null,null,"Source: 6http://www.epa.gov/otaq/models/nonrdmdl/nonrdmdl2010/420r10018.pdf"]
[]
[]
["Off-Road Spark Ignition: Diesel"]
["Units\n(Long Name)","Units","Ratio",null,"Horsepower (hp)","Tier","BSFC (lb/hp*hr)","HC","CO2"]
["Gallons","Gal",1,null,null,null,null,"(g/hp*hr)","(g/gal)"]
["Liters","L",{"$f":"1/3.78541178","v":0.26417205263729593},null,"0 to 11","Tier 0",0.40799999999999997,1.5,{"$f":"(G446*453.6-H446)*0.87*(44/12)/0.367","v":1595.5980163487739}]
[null,null,null,null,null,"Tier 1",0.40799999999999997,0.76280000000000003,{"$f":"(G447*453.6-H447)*0.87*(44/12)/0.367","v":1602.0058310626705}]
[null,null,null,null,null,"Tier 2",0.40799999999999997,0.55079999999999996,{"$f":"(G448*453.6-H448)*0.87*(44/12)/0.367","v":1603.8485558583109}]
[null,null,null,null,null,"Tier 4",0.40799999999999997,0.55079999999999996,1603.8485558583109]
[null,null,null,null,"11 to 25","Tier 0",0.40799999999999997,1.7,1593.8595967302456]
[null,null,null,null,null,"Tier 1",0.40799999999999997,0.438,1604.8290245231608]
[null,null,null,null,null,"Tier 2",0.40799999999999997,0.438,1604.8290245231608]
[null,null,null,null,null,"Tier 4",0.40799999999999997,0.438,1604.8290245231608]
[null,null,null,null,"25 to 50","Tier 0",0.40799999999999997,1.8,1592.9903869209809]
[null,null,null,null,null,"Tier 1",0.40799999999999997,0.27889999999999998,1606.2119373297007]
[null,null,null,null,null,"Tier 2",0.40799999999999997,0.27889999999999998,1606.2119373297007]
[null,null,null,null,null,"Tier 4",0.40799999999999997,0.13139999999999999,1607.4940217983651]
[null,null,null,null,"50 to 75","Tier 0",0.40799999999999997,0.99,1600.0309863760217]
[null,null,null,null,null,"Tier 1",0.40799999999999997,0.52129999999999999,1604.1049727520438]
[null,null,null,null,null,"Tier 2",0.40799999999999997,0.36720000000000003,1605.4444250681197]
[null,null,null,null,null,"Tier 4",0.40799999999999997,0.13139999999999999,1607.4940217983651]
[null,null,null,null,"75 to 100","Tier 0",0.40799999999999997,0.99,1600.0309863760217]
[null,null,null,null,null,"Tier 1",0.40799999999999997,0.52129999999999999,1604.1049727520438]
[null,null,null,null,null,"Tier 2",0.40799999999999997,0.36720000000000003,1605.4444250681197]
[null,null,null,null,null,"Tier 3",0.40799999999999997,0.18360000000000001,1607.040294277929]
[null,null,null,null,null,"Tier 4",0.40799999999999997,0.13139999999999999,1607.4940217983651]
[null,null,null,null,"100 to 175","Tier 0",0.36699999999999999,{"$f":"0.68","v":0.68},1441.0733732970027]
[null,null,null,null,null,"Tier 1",0.36699999999999999,{"$f":"0.3384","v":0.33839999999999998},1444.0425940054495]
[null,null,null,null,null,"Tier 2",0.36699999999999999,{"$f":"0.3384","v":0.33839999999999998},1444.0425940054495]
[null,null,null,null,null,"Tier 3",0.36699999999999999,{"$f":"0.1836","v":0.18360000000000001},1445.3881307901904]
[null,null,null,null,null,"Tier 4",0.36699999999999999,{"$f":"0.1314","v":0.13139999999999999},1445.8418583106265]
[null,null,null,null,"175 to 300","Tier 0",0.36699999999999999,0.68,1441.0733732970027]
[null,null,null,null,null,"Tier 1",0.36699999999999999,0.3085,1444.3024877384198]
[null,null,null,null,null,"Tier 2",0.36699999999999999,0.3085,1444.3024877384198]
[null,null,null,null,null,"Tier 3",0.36699999999999999,0.18360000000000001,1445.3881307901904]
[null,null,null,null,null,"Tier 4",0.36699999999999999,0.13139999999999999,1445.8418583106265]
[null,null,null,null,"300 to 600","Tier 0",0.36699999999999999,0.68,1441.0733732970027]
[null,null,null,null,null,"Tier 1",0.36699999999999999,0.20250000000000001,1445.2238501362399]
[null,null,null,null,null,"Tier 2",0.36699999999999999,0.16689999999999999,1445.5332888283378]
[null,null,null,null,null,"Tier 3",0.36699999999999999,0.16689999999999999,1445.5332888283378]
[null,null,null,null,null,"Tier 4",0.36699999999999999,0.13139999999999999,1445.8418583106265]
[null,null,null,null,"600 to 750","Tier 0",0.36699999999999999,0.68,1441.0733732970027]
[null,null,null,null,null,"Tier 1",0.36699999999999999,0.14729999999999999,1445.7036539509538]
[null,null,null,null,null,"Tier 2",0.36699999999999999,0.16689999999999999,1445.5332888283378]
[null,null,null,null,null,"Tier 3",0.36699999999999999,0.16689999999999999,1445.5332888283378]
[null,null,null,null,null,"Tier 4",0.36699999999999999,0.13139999999999999,1445.8418583106265]
[null,null,null,null,">750","Tier 0",0.36699999999999999,0.68,1441.0733732970027]
[null,null,null,null,null,"Tier 1",0.36699999999999999,0.28610000000000002,1444.4971907356951]
[null,null,null,null,null,"Tier 2",0.36699999999999999,0.16689999999999999,1445.5332888283378]
[null,null,null,null,null,"Tier 4",0.36699999999999999,0.28149999999999997,1444.5371743869212]
[null,null,null,null,"Source: 6http://www.epa.gov/otaq/models/nonrdmdl/nonrdmdl2010/420r10019.pdf"]