	IOWA DEPARTMENT OF NATURAL RESOURCES

	Sanitary Disposal Project Inspection

	

	Permit #: 
	Page 1

	Facility Name:
County:
	Clinton County Area Solid Waste Agency
Clinton
	Date Last Inspection:
	2008

	 Landfill Director:
	Brad Seward
	
	

	Address :
Phone:
	4292 – 220th St., Clinton, IA 52733
563-243-4749 ext 101
	Date This Inspection:
	12/23/09

	
	
	
	

	Responsible Official:
	Same as above
	Waste Amount:  
	~145 T/D

	Address:
Phone: 
	Same as above
Save as above
Burlington, 
	
	

	At the Time of this Inspection:

	· facility personnel present: Josh Christensen – Progress Contracts employee
· active unit(s): Phase 0
	· surface conditions: snow covered
· ambient temperature: ~34 ˚F
· wind direction and speed: E @ ~15-20mph 

	Yes – compliance was being achieved; No – compliance was not being achieved,

N/A – not applicable or not observed; PND – previously noted deficiency (PND).
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	Comments: See next pages for comments.  

	

	INSPECTOR
	Kurt Levetzow
	

	REVIEWER
	Paul Brandt
	


General Description:  Permitted service area includes: all cities & unincorporated area in Clinton County. 
Record Keeping:

1. Inspection records, training procedures, and notification procedures required [See 113.11(1)“d”] During this inspection, the proper personnel capable of providing records were not on site due to vacation or the holidays.  Mr. Seward has provided several records for review via e-mail.  A follow up onsite visit will be conducted, at which time; a comprehensive records review will take place.  
Operating Procedures: 
1. All-weather access roads to the facility [See 113.7(3) “a”]: Yes
2. Controlled access into and within site [See 113.8(3) “a”]: Access to entrance to the landfill is controlled via lockable gate.
- Including a perimeter fence with a lockable gate(s) to help prevent unauthorized access [See    

      113.7(3) “b”]: Yes
3. A sign at the entrance to the facility specifying:  [See 113.7(3) “c”]:

(1) Name and permit number of the facility: Yes

(2) Days and hours that the facility is open to the public or a statement that the facility is not open to the public: Yes

    (3) A general list of materials that are not accepted: Yes

(4) Telephone number of the official responsible for operation of the facility and the emergency contact person(s): Yes
4. All-weather access roads within the facility.  [See 113.7(3) “d” and 113.8(3)”c”]: Interior roads were in excellent condition.
5. A scale certified by the Iowa department of agriculture and land stewardship.  [See 113.7(3)“g” and 113.8(3)”b”]: Yes
6. Waste screening for prohibited materials [See 113.8(1)“a”]:

(1) Random inspections of incoming load: Waste loads are visually screened at the working                

                    face.

(2) Records of any inspections: Have not been recording random inspections.  

(3) Training of personnel to recognize prohibited wastes: Reportedly complying with this      

                         requirement.

(4) Notification to EPA for hazardous wastes: N/A
7. Prohibited materials list [See 113.8(1)“b”]: It is recommended that landfill staff review list prohibited materials as listed in 113.8(1)”b”. 
8. Open burning and fire hazards [See 113.8(1) “c”]: Open burning onsite is prohibited by the Clinton County Landfill as well as 567 IAC 113 & 23.  
9. Animal feeding and grazing [See 113.8(1) “e”]: No animal grazing takes place at the landfill.
10. Working face controlled [See 113.8(2) “d”]: The working face appeared to be ~1 acre in size, at least that is the size of area that was being covered with ADC (msw compost) at the time of this inspection.  The working face shall be no larger than necessary to accommodate the rate of disposal in a safe and efficient manner.  At least one area of the working face did not appear to comply with 113.8(2)”d”(2) – the working face shall not be so steep as to cause heavy equipment and solid waste collection vehicles to roll over or otherwise lose control.  I did not observe evidence that any vehicles rolled over or lost control, however, due to the steepness, waste had not been covered or properly compacted.  This area of the working face was located on the SE corner, the waste was clearly not compacted or covered since the last snowfall which had occurred a couple of days prior to this inspection.                                                                                                                                                                
11. Leachate seeps controlled [See 113.8(2) “g”]: A potential leachate seep was observed during this inspection, located in the closed portion of the landfill, north of the scalehouse, and on the far eastern edge of the property line.  Even though it was raining at the time of this inspection, appearance and odor indicated it was a leachate seep.  Leachate seeps in that area had been an ongoing issue for many years.  567 IAC 113.8(2)”g” states that leachate seeps shall be contained and plugged upon being identified and that the leachate must not reach a water of the state.  During an upcoming follow up visit in January 2010, this area will be re-evaluated.
12. Cover/Alternative cover material adequate [See 113.8(2) “f”]: The use of ADC (msw compost) appeared to be the primary cover material being used during the 12/23/09 inspection on Phase 0.  Use of a soil mixture (at a 50% mix rate with the ADC) was not observed.  The onsite stock-pile of dirt, located near the fuel barrels, was clearly not being accessed, and had not been since the last snow fall, which occurred 1-2 days prior to this inspection.  Therefore, future use of msw compost as ADC must be mixed with soil.  All waste material received at the landfill must be covered at the end of every working day.  Records show that asbestos waste received at the landfill on 9/10/09 & 11/24/09 had not been covered as of 12/23/09.  Also, 55-gallon drums of wax had been left uncovered for approximately one month.  As of 12/28/09, according to Mr. Seward, the materials had been covered.       
13. Litter control [See 113.8(3) “f”]: Due to a strong eastern wind during this inspection, windblown litter was observed caught in a fence ~200 yards west of Phase 0.  Additional litter fencing should be placed on the western edge of active fill areas.  Litter fence is in place on the eastern side of Phase 0.  Litter did not appear to be a problem around the rest of the landfill.  
14. Mud control [See 113.8(3) “h”]: Mud was not observed on the paved areas. 
15. Leachate collection [See 113.7(5)”b”] and treatment [See 113.8(3) “i”]: Leachate is collected, and pumped to the local WWTP.
SUMMARY OF REQUIREMENTS
1. Maintain the working face only large enough to accommodate the rate of disposal in a safe and efficient manner.

2. Cover all waste at the end of every working day, with the appropriate amount of cover material.
3. If ADC is used, incorporate soil with the ADC material at a rate of 50-50.  

4. When leachate seeps are found, either repair as soon as possible or develop a plan of action with a detailed schedule for repair.
5. Remove trees and other deep rooted vegetation from areas with final cover.   

6. Document random load inspections.  
SUMMARY OF REMINDERS

1. All waste, including C&D only working faces, must be covered every day (as opposed to the old 113 rules that allowed for weekly covering of C&D). 
SUMMARY OF RECOMMENDATIONS

1. It is recommended that landfill staff review 567 IAC 113.8(1)“b” (list of prohibited materials).
2. Install a litter fence on the westerly side of the working face.  
3. Locate erosion seeps when they are small and repair them as necessary so as to not have major erosion ruts to deal with all at once.   
