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	Sanitary Disposal Project Inspection

	

	Permit #: 
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	Facility Name:
County:
	Des Moines County Landfill
Des Moines
	Date Last Inspection:
	2008

	 Landfill Manager:
	Eric Houtz
	
	

	Address :
Phone:
	13758 Washington Rd, W. Burlington
319-759-4083
	Date This Inspection:
	12/1/09

	
	
	
	

	Responsible Official:
	Hal Morton
	Waste Amount:  
	200 T/D

	Address:
Phone: 
	1818 West Burlington Avenue
319-753-8126
Burlington, 
	
	

	At the Time of this Inspection:

	· facility personnel present: Eric Houtz, Landfill Manager
· active unit(s):Cells 3&4
	· surface conditions: slightly wet, but drying rapidly
· ambient temperature: 45-50 ˚F
· wind direction and speed: SW@ ~10mph 

	Yes – compliance was being achieved; No – compliance was not being achieved,

N/A – not applicable or not observed; PND – previously noted deficiency (PND).
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	Comments: See next pages for comments.  

	

	INSPECTOR
	Kurt Levetzow
	

	REVIEWER
	Paul Brandt
	


General Description:  Permitted service area includes: all cities & unincorporated area in Des Moines County; Mt. Pleasant, Mt. Union, New London, Rome, Salem, Westwood, and Winfield in Henry County; and Morning Sun in Louisa County.  
Record Keeping:

1. Inspection records, training procedures, and notification procedures required [See 113.11(1)“d”] During this inspection, records of random load inspections were not available for review.  Operators are said to be knowledgeable of what is and is not acceptable in the working face, however, regulations require that documentation of these random load inspections are kept available for inspection.
Operating Procedures: 
1. All-weather access roads to the facility [See 113.7(3) “a”]: Yes
2. Controlled access into and within site [See 113.8(3) “a”]: Access to entrance to the landfill is controlled via lockable gate.
- Including a perimeter fence with a lockable gate(s) to help prevent unauthorized access [See    

      113.7(3) “b”]: It is doubtful the entire perimeter of the facility is fenced off, however, due to    

      the nature of the terrain, unwanted access is next to impossible other than via foot.   
3. A sign at the entrance to the facility specifying:  [See 113.7(3) “c”]:

(1) Name and permit number of the facility: Yes

(2) Days and hours that the facility is open to the public or a statement that the facility is not open to the public: Yes

    (3) A general list of materials that are not accepted: This information was not observed on the sign located at entrance to the facility.  If there is not already another sign specifying such information, please ensure that it is posted near the entrance.

(4) Telephone number of the official responsible for operation of the facility and the emergency contact person(s): Yes
4. All-weather access roads within the facility.  [See 113.7(3) “d” and 113.8(3)”c”]: Interior roads were in excellent condition.
5. A scale certified by the Iowa department of agriculture and land stewardship.  [See 113.7(3) “g” and 113.8(3)”b”]: Yes
6. Waste screening for prohibited materials [See 113.8(1) “a”]:

(1) Random inspections of incoming load: Reportedly complying with this requirement.

(2) Records of any inspections: No records available at time of inspection.

(3) Training of personnel to recognize prohibited wastes: Reportedly complying with this      

                         requirement.

(4) Notification to EPA for hazardous wastes: This information was not requested at time of inspection.
7. Prohibited materials list [See 113.8(1) “b”]: It is recommended that landfill staff review list prohibited materials.
8. Open burning and fire hazards [See 113.8(1) “c”]: Open burning onsite is prohibited by Des Moines County Landfill as well as 567 IAC 113 & 23.  
9. Animal feeding and grazing [See 113.8(1) “e”]: No animal grazing takes place at the landfill.
10. Working face controlled [See 113.8(2) “d”]: Control of working face looked fine.
11. Leachate seeps controlled [See 113.8(2) “g”]: Leachate seeps were not observed during this inspection.
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12. Cover/Alternative cover material adequate [See 113.8(2) “f”]: The C&D working face now needs to be covered daily (the old 113 rules allowed weekly).  Please begin covering C&D daily.  A random follow up visit will be conducted in the next month or two to document compliance with this requirement. 

13. Litter control [See 113.8(3) “f”]: Two employees were out collecting windblown litter at the time of this inspection.  Litter offsite was not observed, and onsite litter has been managed.  Please note, that if litter can not be picked daily, a record of the reason why needs to be maintained per 113.8(3)”f”. 
14. Mud control [See 113.8(3) “h”]: It was reported that mud is periodically scraped off the concrete to keep it from being a runoff or dusting issue.  Mud was not observed on the paved areas. 
15. Leachate collection [See 113.7(5)”b”] and treatment [See 113.8(3) “i”]: Leachate is collected, stored, and hauled to the local WWTP.
General notes:  At the time of the inspection, an outside general contractor was getting ready to scoop sediment out of the sediment pond.  The PCS area appeared to have been disked recently.  Composting area appeared to be in good shape.    
SUMMARY OF REQUIREMENTS
1. Maintain records of random load inspections.  
2. Cover C&D waste daily instead of weekly.
SUMMARY OF REMINDERS

      N/A
SUMMARY OF RECOMMENDATIONS

1. It is recommended that landfill staff review 567 IAC 113.8(1) “b” (see attachment).
