AIR QUALITY COMPLIANCE EVALUATION

COMMENTS

Company Name:
 SSAB Iowa Inc. 
Facility Number:
 70-08-002 
Operating Permit Number:   07-TV-004 
Evaluation Date:
 6/22/10 
GENERAL INFORMATION:
The purpose of this compliance evaluation was to determine the current compliance status of SSAB Iowa Inc (herein referred to as SSAB), with respect to the rules and regulations governing air pollution in the state of Iowa. The scope of this evaluation was limited to a walkthrough inspection of the emission sources, control devices, and any applicable operational and maintenance records.

EP 3, Lime Dolomite Storage Silo – During the facility walk through, white particulate build-up was observed on the top, sides, and near the bottom of the silos, indicating that either over pressurization during transfers from delivery truck to silo, or dust collector malfunction was the culprit.  Please ensure that either way, particulate emissions from such activities are minimized.  

EP 6, Caster Torch – Construction Permit 94-A-553-S3 and SSAB’s TV Permit both limit natural gas usage to ≤ 1,980 scf/hr, however neither permit requires tracking.  SSAB stated that they show compliance with this operating limit as 1,980 scf/hr being the rated capacity of the equipment.  Therefore, Field Office 6 agrees that SSAB can and must show compliance with the limit by maintaining documentation of the equipments rated capacity.     

EP 14, Temperature Retention Units (2) – The construction permit and TV permit limit the maximum natural gas usage for each burner at ≤ 12,950 scf/hr.  SSAB’s natural gas throughput for EP 14 ranged from ~10,000-~14,000 mscf/month.  SSAB stated that 12,950 scf/hr would not be enough fuel to effectively operate the burners.  Therefore, Field Office 6 is requiring that SSAB track natural gas throughput in the units specified in the permit (scf/hr), or request to have the permit modified to reflect unit of measure that suits SSAB’s needs.     
EP 39A-39C, Carbon Injection Silos – Section 14 of the construction permits states the following “the owner or operator shall keep records of control equipment inspection and maintenance”.  During the recordkeeping portion of the evaluation, the inspector failed to request for review the aforementioned records.  Please ensure that SSAB is keeping record of inspections and maintenance for the Carbon Injection Silos.     
REMOVED EQUIPMENT:

· The following two Emission Points were said to have been removed and that their construction permits were rescinded.  According to DNR’s Construction Permit Searchable Webpage, they are still active permits.  If SSAB wishes to rescind the permits, please direct all rescission requests to Kelli Book, Attorney, IDNR Air Quality Bureau, 7900 Hickman Road, Suite 1, Windsor Heights, Iowa 50324.

· EP 36 – Wheelabrator-Shotblast, 04-A-852

· EP 37, 3 Steel Treatment Furnaces, 04-A-853

REQUIREMENTS:

1. Ensure the efficient operation of EP 3’s dust collectors.
2. For EP 14, track natural gas usage in the required units, or apply to have the units modified.

An onsite follow up visit will be conducted within a couple of weeks to review the above listed matters.  
Please note that complying with the above requirement(s) does not in itself preclude the IDNR or US Environmental Protection Agency (USEPA) from initiating enforcement action.

Inspector Initials:   KRL 
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