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On April 22, 2009, I visited the Central Disposal Sanitary Landfill in Winnebago County, Iowa, to observe daily operations.  Ground surface conditions were dry.  There was a northwest wind at 15 mph.  The sky was clear with a temperature near 60°F.  Mike Wick, District Manager, was unavailable at the time of my inspection.  Mr. Ritzert, Certified Operator, accompanied me around the landfill site.  Ms. Moore answered questions concerning the landfill’s records.  
The work area was located on the west part of Phase V.  Daily landfilling in Phase V was progressing from south to north.  Earth was being used for daily cover.  Ms. Moore said the waste received at the landfill averaged about 400 tons per day.  

The daily cover applied several days ago was checked.  Earth cover was marginal at best.  I found many small pockets (2-4 ft. dia.) of exposed solid waste on the cell in question.  Subparagraph 567 IAC 113.8(2) ”f” (1), states, in part, six inches of cover material shall be placed and maintained over the waste in the active portion at the end of each operating day.  The following may help correct this deficiency: maintaining a smaller working face and/or better compaction and/or more cover material.  
Please be advised that the continued application of marginal daily cover increases the possibility of violating the above-referenced cover requirement.  For this reason, daily and intermediate cover will be monitored more closely in the future.
Cathode Ray Tubes (CRTs) were being stored in several trailers.  I asked Mr. Ritzert where the storage area/container was located for damaged CRTs.  Mr. Ritzert said he did not know.  Subrule 567 IAC 122.8(4) requires that CRTs, which show evidence of breakage, leakage, or damage, shall be collected in enclosed and separate containers.  If provisions have not already been made to store damaged CRTs, one must be provided when there are encountered.  
Per the previous inspection requirements, litter control was adequate, and daily cover was still marginal.
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